{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["地面标识标牌"],"not_rendered":{"images":21},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"地面标识标牌","index":0,"n_rows":32,"n_cols":7,"rows_kept":32,"merged":[[0,0,0,6],[1,0,1,6],[3,0,3,6],[10,0,10,6],[18,6,21,6],[31,0,31,4]],"flags":["formulas_cached_only"]}
["三明党校标识、标牌制作"]
["报价单位："]
["序号","材料、设备名称","尺寸(mm)","材质及工艺","数量","报价","图示"]
["户外导视部分"]
[1,"户外总导览图","2500*740*170","1.5不锈钢切割、折弯、围盒、焊接，内置骨架。表面烤漆，立体图案雕刻烤漆，丝印，图案腐蚀雕刻填漆。底座铸件，镀锌圆管烤漆。",4]
[2,"户外车行引导牌","2200*400*170","1.5不锈钢切割、折弯、围盒、焊接，内置骨架。表面烤漆，2mm亚克力红白板立体字，不锈钢围边，内嵌LED防水灯发光，丝印。底座铸件，镀锌圆管烤漆。",6]
[3,"户外人行指引牌","2200*400*170","1.5不锈钢切割、折弯、围盒、焊接，内置骨架。表面烤漆，内容丝印。底座铸件，镀锌圆管烤漆。",6]
[4,"户外多向指引牌","2200*1000圆柱150","1.5不锈钢切割、折弯、围盒、焊接，内置骨架。表面烤漆，内容丝印。底座地图采用不锈钢嵌入地面与地面齐平，信息腐蚀，做旧处理。",8]
[5,"户外宣传公告栏","2200*2600*340","1.5不锈钢切割、折弯、围盒、焊接，内置骨架。表面烤漆，不锈钢精工字雕刻，丝印。图案腐蚀雕刻填漆。8mm透明厢体内置，信息可以更换。",4]
[6,"户外花草牌","750*355*250","1.5不锈钢切割、折弯、围盒、焊接，内置骨架。表面烤漆，内容丝印,立体信息雕刻烤漆。",30]
["户内导视部分"]
[null,"大堂墙面背景字","4500*900*1","不锈钢切割、折弯，电镀古铜金背光,20厚亚克力板",6]
[null,"户内总导览图","1780*1400*1780","1.5不锈钢切割、折弯、围盒、焊接，内置骨架。表面烤白色漆，防指纹处理，图案UV打印,LOGO丝印金色，2mm亚克力图文，信息UV打印。",6]
[null,"楼层索引牌","1250*350*60","1.5不锈钢切割、折弯、围盒、焊接，内置骨架。表面烤白色漆，防指纹处理，图案及面板信息丝印,LOGO丝印金色。",22]
[null,"电梯厅楼层号","305宽  高250","5.0拉丝不锈钢雕刻围边，电镀古铜金,立体字厚度为15mm",113]
[null,"多项指引牌","500*550*5","5.0拉丝不锈钢雕刻围边，电镀古铜金",15]
[null,"科室门牌","230*230","5mm铝板折弯热转印木纹，3mm透明亚克力，信息文字正面丝印，底板",160]
[null,"接待台","4500*1000*600","红色外框侧边，正面白漆背面转印木纹，不锈钢精工字雕刻，电镀古铜金                              (根据原有造型外装)",4]
[null,"洗手间","370*160*50","1.5不锈钢切割、折弯、围盒、焊接，热转印木纹，烤白色漆，图文信息丝印。",18]
[null,"男女","260*80","5mm亚克力雕刻喷漆",44]
[null,"无障碍卫生间","260*80","5mm亚克力雕刻喷漆",11]
[null,"开水间","260*80","5mm亚克力雕刻喷漆",17]
[null,"消防疏散图","250*250","3MM拉丝不锈钢切割，正面烤白色漆转印木纹",122]
[null,"消防楼层号","305宽  高250","5.0拉丝不锈钢雕刻围边，电镀古铜金,立体字厚度为15mm",35]
[null,"公寓门牌","250*250","1.5 拉丝不锈钢切割围盒电镀，古铜金内胆藏LED灯管向下透光，字拉丝不锈钢精工字，电镀古铜金。",799]
[null,"其它门牌（淋浴房，男、女更衣室）","350*1250","5.0拉丝不锈钢雕刻围边，电镀古铜金,立体字厚度为15mm",10]
[null,"设备房牌","250*70","3mm亚克力喷漆，信息丝印,背喷白色漆",201]
[null,"温馨提示牌","150*150","3mm亚克力喷漆，边缘打磨，信息丝印，背喷白色漆",50]
[null,"推拉标识","90*90*3","不锈钢电镀古铜信息丝印",100]
[null,"树牌","60*60*1",null,500]
[null,"石头刻字","个",null,100]
["合计"]